VESSELS NAME - MUSA JALIL

IMO - 8846814

TYPE - SINGLEDECKER

FLAG - RUSSIAN

BUILT - 1989

CLASS - KM \* L4 R2-RSN (4,5)

PANDI CLUB - SOGAZ.

GT/NT - 2554 / 808

SUMMER DWT - 3376MTS

SUMMER DWCC - ABT 3105MTS

DRAFT (SSW) - 3.33 M

GEARED - N/A GEARLESS

LOA/BEAM - 108.4 М/14,8М

GRAIN IN MAIN HOLD - 4383 CBM GRAIN

HOLDS/HATCHES - 4/4

HATCH SIZES -

15.8\*11.2 M

15.8\*11.2 M

15.8\*11.2 M

15.8\*11.2 M

TYPE OF HATCHCOVERS (WHICH TO BE IN GOOD WORKING CONDITION) - MCGREGOR

HORSE POWER - 2\*515 KWT

SERVICE SPEED - ACCORDING TO SHIP’S DOCUMENTS

MAX PRESSURE ON HOLDS BOTTOM - 5,0 MTS/PSQM, ON HATCHES - 1,75 MTS/PSQM

THE AVERAGE SPEED 7.5 KNOTS SUBJECT SEA 2 BEAUFORT

DAILY CONSUMPTION AT SEA (AVERAGE SPEED 7,5 KN, SEA - 2 BEAUFORT): DIESEL OIL (MGO) - 3,5 MT.

DAILY CONSUMPTION IN PORT: DIESEL OIL (MGO) - 0,3 MT

ALL ABOVE MENTIONED IS ABOUT (+/- 5%)

BUNKER-----ISO 8217 2010, MGO SULFUR NOT EXCEED 0,1%