VESSELS NAME - GABDULLA TUKAY

IMO - 8869361

TYPE - SINGLEDECKER

FLAG - RUSSIAN

BUILT - 1986

CLASS - KM\*L4 R2-RSN

PANDI CLUB - SOGAZ

GT/NT - 2829/1012 MT.

SUMMER DWT - 4265 MTS

SUMMER DWCC - 4000 MTS

DRAFT (SSW) - 3.847 M

GEARED - N/A GEARLESS

LOA/BEAM - 105.3 M/ 16.5 M

GRAIN IN MAIN HOLD - 3955 CBM GRAIN

HOLDS/HATCHES - 2/2

HATCH SIZES NR 1 - 28.15\*13.65 M

HATCH SIZES NR 2 - 28.75\*13.65 M

TYPE OF HATCH COVERS (WHICH TO BE IN GOOD WORKING CONDITION) -PULL-WIRE

HORSE POWER - 2X662 KWT

SERVICE SPEED - ACCORDING TO SHIP’S DOCUMENTS

MAX PRESSURE ON HOLDS BOTTOM - 7.0 MTS/ AN HATCHES – 1.7 MTS.

THE AVERAGE SPEED 8 KNOTS SUBJECT SEA 2 BEAU FORT

DAILY CONSUMPTION AT SEA(AVERAGE SPEED 8 KN. SEA – 2 BEAU FORT): DIESEL OIL (MGO) -3,9 MT.

DAILY CONSUMPTION IN PORT: DIESEL OIL (MGO) -0.59 MT.

ALL ABOVE MENTIONED IS ABOUT (+/- 5%)

BUNKER ----IOS. MGO SULFUR NOT EXCEED 0.1%