VESSEL’S NAME - VTS-1

IMO - 8811649

TYPE - GENERAL CARGO

FLAG - RUSSIA

BUILT - 1988

CLASS - КМ \* L4 R2 –RSN

PANDI CLUB - SOGAZ

GT/NT - 1557/467 MT

SUMMER DWT - 1849 T.

SUMMER DWCC - 1740 T.

DRAFT (SWT) - 3.58 M

GEARED - N/A GEARLESS

LOA/BEAM - 82.0 M /11.94 M

GRAIN IN MAIN HOLD - 1820 M3

HOLDS/HATCHES - 2/2

HATCH SIZES №1 - 21.9X9.2 M

HATCH SIZES №2 - 21.4X9.2 M

TYPE OF HATCH COVERS (WHICH TOBE IN GOOD WORKING CONDITION):

HYDRAULICS

HORSE POWER - 2X441 KWT

SERVICE SPEED - ACCORDING TO SHIP’S DOCUMENTS

MAX PRESSURE ON HOLDS BOTTOM – 6.0 MTS/ AN HATCHES – 1.3 MTS

THE AVERAGE SPEED 7.5 KNOTS SUBJECT SEA 2 BEAU FORT

DAILY CONSUMPTION AT SEA (AVERAGE SPEED 7.5 KNOTS SUBJECT SEA 2 BEAU FORT): DIESEL OIL(MGO) – 3.4 MT

DAILY CONSUMPTION IN PORT: DIESEL OIL (MGO) - 0.432 MT

ALL ABOVE MENTIONED IS ABOUT (=/- 5%)

BUNKER ---- IOS. MGO SULFUR NOT EXCEED 0.1%